# Trek iets ordentlik aan
### The Allrounder Steel toe cap – ISO 20345 approved
Perfect for people who are always on the move Steel toe cap – ISO 20345 approved Manufactured with a double layer of leather (2.2mm full-grain leather, lined with 1.6mm calf leather) A steel shank between the insole board and sole offers extra support and stability The insole board is secured to the upper with a double stitched 2.2mm braided nylon cord Accommodates a wider foot with a roomy toe box Sole is made from a genuine rubber Can be resoled
Kliek op die logo vir meer skoene
Klick on the logo for more shoes