Patented anti-grab design. Built for SPF and SAF. ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌ ‌

Words I like: Control isn't about strength. It's about design. Hey ! Your Light Is Easy to Grab Most duty flashlights have a design problem nobody thinks about until it matters. To press the tail button, you shift your grip. Your palm opens up. For a fraction of a second, the light isn't fully secure in your hand. During a routine walkthrough, that's nothing. During a confrontation, that's how you lose your light. It happens because most flashlights were designed for people standing still. The buttons are positioned for convenience, not retention. Every time you switch modes, you're choosing between operating the light and holding onto it. The new P27iX was designed around that problem.
The angled rear control surface keeps your thumb on both tail buttons at once. You switch between momentary and sustained output without re-gripping, without opening your palm. It's a patented design, built for gloved use, quick draws, and situations where retention actually matters. And the rest of the light is built the same way. Three beam patterns, switchable mechanically: focused throw at 430 metres, 115-degree flood for room clearing, and mixed beam for patrol. Each brightness level remembers your beam setting, so you configure it once and it stays. No menus during a building check. Two programmable grip profiles: Tactical Grip for response and entry, Duty Grip for routine work. Both press stages on each tail button are independently configurable. Your light matches your unit's procedure, not the other way round. 5,000 lumens from 20 LED cores. Pure white beam, no green tint at any output. 7075-T6 aerospace aluminium. IP68 to 2 metres. Ceramic strike bezel for glass breaking. CR123 backup magazine for deployment. Mechanical lockout so it doesn't fire in your holster. 143mm, 201g with battery. Built for SPF, SAF, auxiliary police, and licensed security operators. As promised, value in under a minute. The P27iX just landed in Singapore. First batch is 50 units. Use Code 60off takes $60 off at checkout, bringing it to $199. Code expires 16 May or when the batch sells out, whichever comes first: Grab yours here with the discount applied. 60-day money-back guarantee. Keep the grip. Keep the light. Sincerely, Ming Jie Nitecore Singapore P.S. My old flashlight bouncing off the floor mid-demo.

You're getting this email because you opted in on our website or have bought something from us before. Prefer to be left out? . Nitecore Singapore Pte Ltd. 5008 Ang Mo Kio Avenue 5, #04-09/16, TechPlace II, Singapore 569874